{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.03","0.03"]
["","Hагрев","","Ном.","кВт","0.035","0.035"]
["Корпус","Цвет","","","","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","285","285"]
["","","","Ширина","мм","770","770"]
["","","","Глубина","мм","225","225"]
["Масса","Блок","","","кг","9","9"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","10.6","11.4"]
["","","","Средн.","м³/мин","7.7","8.2"]
["","","","Низк.","м³/мин","5.3","5.4"]
["","","","Тихая работа","м³/мин","4.3","4.3"]
["","","Hагрев","Выс.","м³/мин","11.2","10.8"]
["","","Нагрев","Средн.","м³/мин","8","7.8"]
["","","Hагрев","Низк.","м³/мин","5.8","5.8"]
["","","","Тихая работа","м³/мин","4.9","4.9"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","58","58"]
["","Отопление","","","дБ(A)","58","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","43","43"]
["","","","Средн.","дБ(A)","35","35"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","26","26"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","21","21"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","43","43"]
["","Нагрев","","Средн.","дБ(A)","35","35"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","26","26"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","21","21"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5"]
["","Дренаж","","","","16 (внутренний диаметр соединительного шланга)","16 (внутренний диаметр соединительного шланга)"]
["Системы управления","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Электропитание","Наименование","","","","V1","V1"]
["","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-240","220-240"]