{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVX-D6VG / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","EAVX16S18DA6VG / EPGA11DAV3","EAVX16S23DA6VG / EPGA11DAV3","EAVX16S18DA6VG / EPGA14DAV3","EAVX16S23DA6VG / EPGA14DAV3","EAVX16S18DA6VG / EPGA16DAV3","EAVX16S23DA6VG / EPGA16DAV3"]
["ГВС","Общие сведения","Гарантированная нагрузка","","L","XL","L","XL","L","XL"]
["","Среднеклимат. условия","Класс энергоэффективности нагрева воды","","A","A","A","A","A","A"]
["COP","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Внутренний блок","","","","EAVX16S18DA6V","EAVX16S23DA6V","EAVX16S18DA6V","EAVX16S23DA6V","EAVX16S18DA6V","EAVX16S23DA6V"]
["Холодопроизводительность","Ном.","","кВт","10.5 (1), 10.7 (2)","10.5 (1), 10.7 (2)","11.1 (1), 11.9 (2)","11.1 (1), 11.9 (2)","13.5 (1), 11.9 (2)","13.5 (1), 11.9 (2)"]
["EER","","","","4.75 (1), 3.23 (2)","4.75 (1), 3.23 (2)","4.09 (1), 2.99 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Теплопроизводительность","Ном.","","кВт","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Потребляемая мощность","Охлаждение","Ном.","кВт","2.21 (1), 3.30 (2)","2.21 (1), 3.30 (2)","2.72 (1), 3.97 (2)","2.72 (1), 3.97 (2)","3.42 (1), 3.97 (2)","3.42 (1), 3.97 (2)"]
["","Hагрев","Ном.","кВт","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Примечания","","","","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]