{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-PAV3"]
[]
[]
[]
[]
["","","","","","EKHH2E260PAAV3"]
["Sound power level","Нагрев для ГВС","","Внутренний блок","дБ(A)","53"]
["","","","Наружный блок","дБ(A)","52"]
["Нагрев для ГВС","Общие сведения","","Класс энергоэффективности нагрева воды","","A+"]
["","","","Установка темп. термостата","°C","55"]
["","","","Гарантированная нагрузка","","XL"]
["","Холодноклимат. условия","","AEC (Годовое потребление электроэнергии)","кВтч","1,826"]
["","Теплоклимат. условия","","AEC (Годовое потребление электроэнергии)","кВтч","1,296"]
["","Среднеклимат. условия","","AEC (Годовое потребление электроэнергии)","кВтч","1,323"]
["Эквивалент горячей воды","Макс.","","","л","342"]
["Тепловой насос","Automatic defrost start","","","°C","-2"]
["","Рабочий диапазон","Темп. нар. возд.","Мин.","°C сух.т.","-7"]
["","","","Макс.","°C сух.т.","38"]
["","Casing","","Material","","Крышка: Обработка верхней части EPP (вспенивающийся полипропилен)"]
["","","","Цвет","","White body / black top"]
["","Давление системы","","Макс.","бар","7"]
["","Способ разморозки","","","","Активный, с клапаном для горячего газа"]
["COP","","","","","3.10 (1), 3.60 (2)"]
["Хладагент","ПГП","","","","1,430.0"]
["","Charge","","","кг","0.900"]
["","Тип","","","","R-134a"]
["Compressor","Тип","","","","Rotary non-inverter"]
["Размеры","Блок","","Диаметр","мм","650"]
["","","","Высота","мм","2,000"]
["ГВС","Выход","","Ном.","кВт","1.8"]
["Бак","Установка","","Возможность подключения к солнечным коллекторам","","Да"]
["","Мощность встроенного теплового элемента","","Ном.","кВт","1.5"]
["","Корпус","","Материал","","Тисненый ABS (акрилонитрил-бутадиен-стирол)"]
["","","","Цвет","","Белый"]
["","Размеры","Блок","Высота","мм","1,500"]
["","Рабочий диапазон","Сторона воды","Макс.","°C","56"]
["","","","Мин.","°C","10"]
["Масса","Упакованный блок","","","кг","132"]
["","Блок","","Порожний","кг","112"]
["","","","Полный","кг","358"]
["Место установки","","","","","Внутренний"]
["IP class","","","","","IP-X4"]
["Общие сведения","Описание","","Система воздух-вода с тепловым насосом","","Да"]
["","Реквизиты поставщика/производителя","","Название и адрес","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Время разогрева","Макс.","","","чч:мм","10:14:00, 07:56:46"]
["Тепловой насос","Электропитание","","Частота","Гц","50"]
["","","","Максимальный рабочий ток","A","2"]
["","","","Фаза","","1P"]
["","","","Напряжение","V","230"]
["Бак","Электропитание","","Фаза","","1P"]
["","","","Частота","Гц","50"]
["","","","Напряжение","V","230"]
["Примечания","","","","","(1) - Согласно EN16147-2011, температура на входе 7°C, температура в помещении 20°C, вход холодной воды 10°C"]
["","","","","","(2) - Согласно EN16147-2011, температура на входе 15°C, температура в помещении 20°C, вход холодной воды 10°C"]
["","","","","","(3) - Температура в помещении: 29°CDB, 19°CWB; температура наружного воздуха: 46°CDB, 24°CWB"]
["","","","","","(4) - Температура в помещении: 27°CDB, 19°CWB; температура наружного воздуха: 35°CDB, 24°CWB"]