{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":14,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-KV"]
[]
[]
[]
[]
["","","","","","FTX20K2V1B","FTX20K5V1B","FTX25K2V1B","FTX25K5V1B","FTX35K2V1B","FTX35K5V1B","FTX50K2V1B","FTX60K2V1B","FTX71K2V1B"]
["Входная мощность","Охлаждение","","Ном.","kW","0.018","0.018","0.02","0.02","0.024","0.024","0.035","0.041","0.041"]
["","Hагрев","","Ном.","kW","0.022","0.022","0.023","0.023","0.029","0.029","0.038","0.044","0.044"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","286","286","286","286","286","286","295","295","295"]
["","","","Ширина","мм","770","770","770","770","770","770","990","990","990"]
["","","","Глубина","мм","225","225","225","225","225","225","263","263","263"]
["Масса","Блок","","","кг","8.5","8.5","8.5","8.5","9","9","13.5","13.5","13.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.9","9.9","10.4","10.4","11.8","11.8","16","17.6","17.6"]
["","","","Средн.","м³/мин","7.8","7.8","8","8","8.2","8.2","13.7","14.9","14.9"]
["","","","Низк.","м³/мин","5.8","5.8","6.1","6.1","6.3","6.3","11.1","12.2","12.2"]
["","","","Тихая работа","м³/мин","4.8","4.8","4.8","4.8","4.9","4.9","10.1","11.2","11.2"]
["","","Hагрев","Выс.","м³/мин","10.9","10.9","11.1","11.1","12.8","12.8","16.7","18.9","18.9"]
["","","Нагрев","Средн.","м³/мин","8.5","8.5","8.5","8.5","8.5","8.5","14.7","16.7","16.7"]
["","","Hагрев","Низк.","м³/мин","6.4","6.4","6.7","6.7","6.9","6.9","12.2","13.7","13.7"]
["","","","Тихая работа","м³/мин","5.2","5.2","5.2","5.2","5.2","5.2","10.9","12.1","12.1"]
["Уровень звуковой мощности","Охлаждение","","","дБA","55","55","55","55","58","58","59","60","62"]
["","Отопление","","","дБA","55","55","55","55","58","58","58","59","61"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","39","39","40","40","43","43","43","45","46"]
["","","","Средн.","дБA","33","33","33","33","34","34","39","41","42"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","25","26","26","27","27","34","36","37"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","20","20","20","20","20","20","31","33","34"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39","39","40","40","43","43","42","44","45"]
["","Нагрев","","Средн.","дБA","34","34","34","34","35","35","38","40","41"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","28","28","28","28","29","29","33","35","36"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","23","23","23","23","26","26","30","32","33"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5","9.5","9.5","9.5","12.7","12.7","12.7"]
["","Дренаж","","","","18","18","18","18","18","18","16","16","16"]
["Системы управления","Infrared remote control","","","","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073","BRC944B2, BRC073","BRC944B2, BRC073"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]