{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","43"]
["","","","Средн.","дБA","35"]
["","","","Тихая работа","дБA","21"]
["","","","Низк.","дБA","26"]
["","Охлаждение","","Средн.","дБA","35"]
["","","","Тихая работа","дБA","21"]
["","","","Низк.","дБA","26"]
["","","","Выс.","дБA","43"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Руководство по эксплуатации","","","","1"]
["","Беспроводной пульт дистанционного управления","","","","1"]
["","Сухие батареи AAA","","","","2"]
["","Держатель пульта дистанционного управления","","","","1"]
["","Монтажная пластина","","","","1"]
["","Титано-апатитовый дезодорирующий фильтр","","","","2"]
["","Крепежные винты внутреннего блока","","","","2"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Подсоединение труб","Жидкость","","НД","мм","6.35"]
["","Газ","","НД","мм","9.50"]
["","Дренаж","","","","16 (внутренний диаметр соединительного шланга)"]
["Входная мощность","Охлаждение","","Ном.","kW","0.030"]
["","Hагрев","","Ном.","kW","0.035"]
["Уровень звуковой мощности","Охлаждение","","","дБA","58"]
["","Отопление","","","дБA","58"]
["Размеры","Блок","","Ширина","мм","770"]
["","","","Глубина","мм","225"]
["","","","Высота","мм","285"]
["Корпус","Цвет","","","","Белый"]
["Масса","Блок","","","кг","9.0"]
["Power supply","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Наименование","","","","V1"]
["","Напряжение","","","V","220-240"]
["Примечания","","","","","(1) - Электрические параметры см. в отдельных чертежах"]
["Входная мощность","Охлаждение","","Ном.","kW","","0.03"]
["","Hагрев","","Ном.","kW","","0.035"]
["Корпус","Цвет","","","","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","285"]
["","","","Ширина","мм","","770"]
["","","","Глубина","мм","","225"]
["Масса","Блок","","","кг","","9"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","11.4"]
["","","","Средн.","м³/мин","","8.2"]
["","","","Низк.","м³/мин","","5.4"]
["","","","Тихая работа","м³/мин","","4.3"]
["","","Hагрев","Выс.","м³/мин","","10.8"]
["","","Нагрев","Средн.","м³/мин","","7.8"]
["","","Hагрев","Низк.","м³/мин","","5.8"]
["","","","Тихая работа","м³/мин","","4.9"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","58"]
["","Отопление","","","дБA","","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","","43"]
["","","","Средн.","дБA","","35"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","","26"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","","21"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","","43"]
["","Нагрев","","Средн.","дБA","","35"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","","26"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","","21"]
["Подсоединение труб","Жидкость","","НД","мм","","6.35"]
["","Газ","","НД","мм","","9.5"]
["","Дренаж","","","","","16 (внутренний диаметр соединительного шланга)"]
["Системы управления","Infrared remote control","","","","","ARC480A11"]
["Системы управления","Проводной пульт дистанционного управления","","","","","BRC944B2, BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Электропитание","Наименование","","","","","V1"]
["","Фаза","","","","","1~"]
["","Частота","","","Гц","","50"]
["","Напряжение","","","V","","220-240"]