{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H519K"]
[]
[]
[]
[]
["","","","","BRC1H519K."]
["Упаковка","Материал","","","Тонкий картон"]
["","Вес","","кг","0.0850"]
["Температура наружного воздуха","Относительная влажность <","","%","95"]
["Размеры","Упакованный блок","Ширина","мм","217"]
["","","Высота","мм","50"]
["","","Глубина","мм","161"]
["","Блок","Ширина","мм","85"]
["","","Глубина","мм","25"]
["","","Высота","мм","85"]
["Корпус","Крышка кнопки","","","Нет"]
["","Цвет","","","Black"]
["","СИД работы","Цвет","","Blue status indicator"]
["ЖКИ","Тип","","","100 x 150 dots"]
["","Подсветка","Цвет","","Белый"]
["","Размеры","Ширина","мм","28.0"]
["","","Высота","мм","40.7"]
["Масса","Упакованный блок","","кг","0.317"]
["","Блок","","кг","0.110"]
["Соединительная проводка","Длина проводки","Макс.","м","500"]